Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |  |
| --- | --- | --- |
| Hazard / Regulatory Requirements | ES&H Clause | Worker Information and Requirements |
| Water Boating Activities29 CFR 1926.106 | The Seller shall comply with applicable sections of the Inland and International Navigation Rules as presented by the U.S. Coast Guard and the Tennessee Boating Safety Act. | Workers shall ensure they are experienced and trained to operate watercraft and deploy ring buoy before initiating work on/over water where the danger of drowning exists.Workers shall inspect watercraft and ring buoy before each use and will ensure the ring buoy has at least 90 feet of line.Workers shall ensure they have the required number of personal flotation devices (PFD). Workers shall inspect them before each use and shall wear the PFD when working over or near water where the danger of drowning exists.Workers shall ensure boat safety ignition switch is in working order.Workers shall ensure they use the buddy system when using watercrafts. |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|       |       | **Elimination, substitution, engineering controls**:[ ]  HEPA-Filtered vacuum cleaner [ ]  Laboratory hood or glove box [ ]  Air Handler, HEPA filtered [ ]  Shrouded tool with HEPA filter [ ]  Continuous wetting (dust control) [ ]  Containment[ ]  Isolation [ ]  General Ventilation [ ]  Other Local Exhaust System:      Other: Specify below      |
| **Administrative controls** (work methods, training, medical, etc.):      |
| **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.):      |

AHA Author:       Date:

|  |
| --- |
| Technical Procurement Officer (TPO) signature indicates approval of activity-specific hazard controls identified in the subcontractor AHA. It is recommended that the applicable Qualified Health and Safety Professional (QHSP) be consulted, when the TPO is unfamiliar with the hazard, to assist in reviewing the adequacy of controls specified in this document.Printed Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_  |