Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |  |
| --- | --- | --- |
| Hazard / Regulatory Requirements | ES&H Clause | Worker Information and Requirements |
| Abrasive Wheel Equipment  29 CFR 1910.215 | The Seller shall comply with the requirements of 29 CFR 1910.215. | Worker shall have completed the required training for use of abrasive wheel equipment.  Worker shall ensure the Abrasive Wheel Equipment Program Manager has approved wheel equipment before starting any on site work.  Worker shall ensure that they wear personal protective equipment that is specified in the AHA.  Worker shall NOT use compressed air to clean.  Worker shall ensure all abrasive wheel equipment is mounted between flanges.  Worker shall use exhaust ventilation systems in containment structures to capture dust.  Workers shall vacuum with HEPA filter or remove contaminated work clothes and wash hands before eating, drinking or smoking |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|  |  | **Elimination, substitution, engineering controls**:  HEPA-Filtered vacuum cleaner  Laboratory hood or glove box  Air Handler, HEPA filtered  Shrouded tool with HEPA filter  Continuous wetting (dust control)  Containment  Isolation  General Ventilation  Other Local Exhaust System:  Other: Specify below |
| **Administrative controls** (work methods, training, medical, etc.): |
| **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.): |

AHA Author:       Date:

|  |
| --- |
| Technical Procurement Officer (TPO) signature indicates approval of activity-specific hazard controls identified in the subcontractor AHA. It is recommended that the applicable Qualified Health and Safety Professional (QHSP) be consulted, when the TPO is unfamiliar with the hazard, to assist in reviewing the adequacy of controls specified in this document.  Printed Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_ |