Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |
| --- | --- |
| Hazard / Regulatory Requirements | Main Elements to be Addressed |
| Beryllium  10 CFR 850  29 CFR 1910.1024, permissible exposure limit (PEL) ONLY | Workers shall ensure they are Beryllium trained and enrolled in their Company’s beryllium medical surveillance program.  Workers shall immediately contact Industrial Hygiene for questions with beryllium work.  Work with potential for exposure to or contact with beryllium is conducted under an approved Beryllium Exposure Prevention Plan (BEPP).  Workers shall ensure they comply with requirements specified in the BEPP. This includes wearing of personal protective equipment specified in the BEPP.  Workers shall ensure Beryllium waste is labeled. |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|  |  | **Elimination, substitution, engineering controls**:  HEPA-Filtered vacuum cleaner  Laboratory hood or glove box  Air Handler, HEPA filtered  Shrouded tool with HEPA filter  Continuous wetting (dust control)  Containment  Isolation  General Ventilation  Other Local Exhaust System:  Other: Specify below |
|  |  | **Administrative controls** (work methods, training, medical, etc.): |
|  |  | **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.): |
| **USE THE SPACES BELOW TO COMPLETE SIMILAR AHAs FOR OTHER HAZARDS ASSOCIATED WITH THIS ACTIVITY** | | |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Use the Activity Hazard Analysis Continuation Sheet if additional lines are needed.**

AHA Author:       Date:

ES&H/QHSP Representative Concurrence signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_

|  |
| --- |
| Technical Procurement Officer signature indicates approval of activity-specific hazards controls identified in the subcontractor AHA.  Print Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_ |