Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |  |
| --- | --- | --- |
| Hazard / Regulatory Requirements | ES&H Clause | Worker Information and Requirements |
| Diving  29 CFR 1910, Commercial Diving Operations | The Seller shall comply with the requirements of 29 CFR 1910, Subpart T, Commercial Diving Operations. | Workers shall ensure they have the experience and training necessary to perform assigned diving tasks in a safe and healthful manner.  Workers shall be medically cleared as a diver and must use the buddy system.  Workers shall ensure they have the experience and training to use and operate tools, equipment, and diving systems relevant to the assigned tasks, and shall not conduct diving operations unless an assigned person-in-charge is present at the dive site.  Workers shall be trained and in emergency procedures.  Workers shall contact LSS Office (865.576.4LSS) in the event of a fuel, oil or hydraulic fluid spill or in the event of an emergency. |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|  |  | **Elimination, substitution, engineering controls**:  HEPA-Filtered vacuum cleaner  Laboratory hood or glove box  Air Handler, HEPA filtered  Shrouded tool with HEPA filter  Continuous wetting (dust control)  Containment  Isolation  General Ventilation  Other Local Exhaust System:  Other: Specify below |
| **Administrative controls** (work methods, training, medical, etc.): |
| **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.): |

AHA Author:       Date:

|  |
| --- |
| Technical Procurement Officer (TPO) signature indicates approval of activity-specific hazard controls identified in the subcontractor AHA. It is recommended that the applicable Qualified Health and Safety Professional (QHSP) be consulted, when the TPO is unfamiliar with the hazard, to assist in reviewing the adequacy of controls specified in this document.  Printed Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_ |