Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |  |
| --- | --- | --- |
| Hazard / Regulatory Requirements | ES&H Clause | Worker Information and Requirements |
| ErgonomicsAmerican Congress of Industrial Hygienist Threshold Limit Values for Ergonomic hazards, 2005 edition | Prior to the commencement of any on-site work, methods to identify and prevent work-related musculoskeletal disorders shall be developed and implemented by the Seller. Seller shall provide documentation to the ORNL site safety contact upon request. | Workers shall be aware of ergonomic hazards, such as tasks that require exertion of high force, awkward posture or position, high repetition, vibration, or prolonged static posture, and of methods to minimize those hazards.Workers shall understand their individual physical capabilities for manual material handling and do not perform work beyond their physical limitations. Workers shall provide documentation of methods employed to identify and prevent work-related musculoskeletal disorders to the Technical Project Officer and/or Site Safety representative prior to starting any on-site work. |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|       |       | **Elimination, substitution, engineering controls**:[ ]  HEPA-Filtered vacuum cleaner [ ]  Laboratory hood or glove box [ ]  Air Handler, HEPA filtered [ ]  Shrouded tool with HEPA filter [ ]  Continuous wetting (dust control) [ ]  Containment[ ]  Isolation [ ]  General Ventilation [ ]  Other Local Exhaust System:      Other: Specify below      |
| **Administrative controls** (work methods, training, medical, etc.):      |
| **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.):      |

AHA Author:       Date:

|  |
| --- |
| Technical Procurement Officer (TPO) signature indicates approval of activity-specific hazard controls identified in the subcontractor AHA. It is recommended that the applicable Qualified Health and Safety Professional (QHSP) be consulted, when the TPO is unfamiliar with the hazard, to assist in reviewing the adequacy of controls specified in this document.Printed Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_\_\_\_\_  |