Subcontractor Name:       Project Title and Subcontract Number:

Description of planned activities/tasks for the scope-of-work for the entire project.

|  |  |
| --- | --- |
| Hazard / Regulatory Requirements | Main Elements to be Addressed |
| Through Penetration of Fire Barrier | Workers shall ensure the fire stop system has been approved by the Subject Matter Experts at the COMPANY. The Technical Project Officer shall be contacted with questions or concerns.Workers shall install penetration systems as tested in an approved fire-resistance-rated assembly.Workers shall contact LSS Office (865.576.4LSS) in the event of an accident/emergency. |

**Subcontractor Activity Hazard Analysis (AHA)**

| Activity | Hazard | Controls |
| --- | --- | --- |
|       |       | **Elimination, substitution, engineering controls**:[ ]  HEPA-Filtered vacuum cleaner [ ]  Laboratory hood or glove box [ ]  Air Handler, HEPA filtered [ ]  Shrouded tool with HEPA filter [ ]  Continuous wetting (dust control) [ ]  Containment[ ]  Isolation [ ]  General Ventilation [ ]  Other Local Exhaust System:      Other: Specify below      |
|  |  | **Administrative controls** (work methods, training, medical, etc.):      |
|  |  | **Personal protective equipment** - specify the exact type of PPE (e.g. hearing protection device with minimum NRR of 20 dBA, Ansell Nitrile SOL-VEX gloves, etc.):      |

**For additional activities/tasks or hazards, use an AHA continuation sheet.**

AHA Author:       Date:

|  |
| --- |
|  Technical Procurement Officer signature indicates approval of activity-specific hazards controls identified in the subcontractor AHA.Print Name/Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date\_\_\_\_\_\_\_\_\_ |